Machine Maintenance

[Manual for Multiheads (TMAR-K)](http://docs.hic.us/i/445658-tmark-instruction-7-2014)

Oiling your machines

[Tajima Instructional video](https://youtu.be/ZLDVMSFV2Rc)

[Megan’s Monday routine](https://youtu.be/rA4ki3x-R-w)

[Ricoma Video of daily and weekly care](https://youtu.be/wAfxu4oT3vs) - Watch first 2.5 min.

Changing a Needle and Choosing the right one for the job

[Changing Thread color through Tajima menu mid file](https://youtu.be/fm3BF8KEG9o)

[Removing the Shipping stabilizer bracket from the head after transport (Video).](https://www.youtube.com/watch?v=GFyN8ZxaQ2c&feature=youtu.be)

Troubleshooting guides

2CE-00 Safety Sensor - [Video on troubleshooting](https://youtu.be/QtP3YVs4KxU)

2E3 - Power issue, turn off for 10 sec and turn back on. Another issue might have caused this to pop up and this is a bigger system restart to correct the original issue.

316 - Frame Issue - Turn off and on. Try thread color change and manual thread cut. Turn dial to unstick the part jammed up.

36A- 00 movable knife open - [How to fix Front of Machine](https://youtu.be/NVIku-9nOXU), [How to fix Back of Machine](https://youtu.be/gqbGlUjQPL4)

5C1-30 Need to recenter calibration - [Video on how to fix](https://youtu.be/IRarZ59twKc)

Sounds:

Knocking metal on metal - Try Oiling first, then Call Hirsh